This version is V1.1.0.1 has
1) Minor bug fixes in the vector driver and other driver selection and status info display in the status box.

This is the version 1.1.0.0 which has 
1) Drivers : CAN, USB

2) Protocols : MQTT, HTTP, HTTPS
	a) HTTP and HTTPS just uploads the file to server in regular fashion without UDS proto. 

3) USB driver now has a connect() API with VID, PID and also specify the driver selection whether its for USB or CAN , passed as paramenters along with wheather the driver should be used as purely USB for raw usb data reception OR USB for reception of CAN frames.

4) version 2.6.1.0 
	USB and Serial driver Disable. ONly SBUSCAN (inside CAN) is Enable 
	setup file path: 